	091-55-15-DC-24
	Super 15 Auto Eject, 240 Vac, 15 Amp, 24 Vdc


EJECTION UNIT
A Kussmaul Super Auto Eject Model #091-55-15-DC-24, 15 amp, 240 Vac, 24 Vdc shore power assembly, cover, solenoid input wire, power cord, and plug shall be installed.   The 24 volt solenoid shall eject the shore power cord away from vehicle path upon sensing engine start; after ejection, the weatherproof cover snaps into position over inlet. The unit shall sequence energizing of an Auto Eject, eliminating terminal arching when connecting and disconnecting power cord.  
The unit shall have a waterproof back enclosure with watertight cable fittings, which protect mechanism from road contamination.  A pre-wired 3 foot AC electrical cord and starting sense wire (side wired) shall be installed.   

The assembly shall have the following dimensions: 6.17” high x 4.08” wide x 2.8” deep with 4 lb. weight.   Color of cover shall be:  (yellow) (red) (blue) (white) (gray) (black)
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